laminarflow_to              .35
laminarflow_cruise          .50
laminarflow_loiter          .50
laminarflow_landing         .35


M_cruise            0.8
M_to                0.2509
M_loiter            0.3
M_landing           0.28

cLalpha             0.037
cL0                 0.0845
cMalpha             0.0003
cM0                 -0.0369

efficiency_to       0.7781
efficiency_cruise   0.98
efficiency_loiter   0.9692
efficiency_landing  0.8791

alt_cruise          35000
alt_to              0
alt_loiter          10000
alt_landing         0

weight_cruise       173400
weight_to           173400
weight_loiter       133900
weight_landing      133900

cd_correction       0
c_f                 0.003
D_engine            240.5
fuse_width          57.96
Dragredux_BLI       5.7
sfront_landinggear 33.7
cd_landinggear     .4